Manual
Turn off the printer status
While holding down the panel "CD Tray" key and the center of the touch screen

(Red dots illustrated position), then hold down the switch "ON" button, three keys simultaneously for 3 seconds into the Firmware Upgrade mode:
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LCD screen as shown below:
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Computer prompts discovery of new hardware, click Cancel,
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Program runs inside Reset.exe
[image: image8.png][

e





Click “1st ROM File“Designation  TX800PX800A800dat
Folder, select FWA539TL1.dat File
Click “2nd ROM File“Designation TX800PX800A800dat
Folder, select FWA539TL2.dat File
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Then click "Transfer" button

At this point the data transmitted to the printer firmware

Firmware printer LCD screen correctly transmitted in turn displays the following information: (**: changes in the transmission process on behalf of readings)
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Two Firmware files sequentially written in the ROM1 and ROM2, time is about 2 minutes.
Upon completion of the full LCD screen button is highlighted below：
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Press the panel "CD Tray" button, the printer automatically shutdown, Firmware upgrade is complete
The printer has become TX800 printer
Then use ordinary TX800-RESET.rar cleared software printer can be cleared
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If the printer is not properly connected to the computer will display as shown above

Information, Firmware upgrade will not continue, please check the USB printer connection, restart the printer, the computer attempts to re-


Ensure proper receiving my mail
Use Google Mail or MSN mail
My e-mail address used
Reset999@msn.com
1915611409@qq.com
Requirements? Help? Please send an e-mail
